driverless(1)

NAME
driverless - PPD generator utility for driverless printing

SYNOPSIS
driverless [-h | --help | --version] [-d | -v | --debug] [list] | [cat driver URI] | [IPP printer URI]

DESCRIPTION
driverless generates PPD files for printers which are designed for driverless IPP printing (currently IPP Everywhere, AirPrint, Mopria, and Wi-Fi-Direct printers, network printers and also IPP-over-USB printers with the help of ippusbxd(8)) by polling capability information from the printers via IPP. it can be either called for listing suitable printers in the network and for actually generating the PPD. It can also be called by CUPS when CUPS is listing available PPDs/drivers or creating print queues, making the setup of driverless printers with printer setup tools transparently working.

driverless is placed in /usr/lib/cups/driver/ for listing available driverless-capable printers and generating PPDs for them. It should also be put in /usr/lib/cups/backend/ (preferably by a symbolic link) to list IPP device URIs for suitable printers. Printer setup tools like system-config-printer, the CUPS web interface at http://localhost:631/, and CUPS' command line utilities can use driverless with CUPS to list available driverless-capable printers, determine their IPP device URIs and generate PPDs for them. The printers will be automatically and correctly set up for driverless printing. Note that driverless printing requires IPP communication with the printer.

A second symbolic link to /usr/lib/cups/driver/driverless from /usr/bin/ allows driverless to be called directly by a user.

OPTIONS

-h, --help, --version
    Show help page, including version number.

-v, -d, --debug
    Debug mode, verbose logging to stderr.

list
    List the driver URIs and metadata for all available IPP printers suitable for driverless PPD file generation (to be used by CUPS).

cat driver URI
    Generate the PPD file for the supplied driver URI from the output of "list" (to be used by CUPS).

IPP printer URI
    Generate the PPD file for the supplied IPP printer URI (suitable URIs are listed when calling driverless without options).

When called without options, the IPP printer URIs of all available driverless-capable IPP printers will be listed.

SEE ALSO
cups-browsed(8), ippfind(1), ippusbxd(8)

AUTHOR
The authors of driverless are listed in /usr/share/doc/cups-filters/AUTHORS.